EHDS Logical Information Models
0.2.1 - qa-preview

EHDS Logical Information Models, published by Xt-EHR. This guide is not an authorized publication; it is the continuous build for version 0.2.1 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/Xt-EHR/xt-ehr-common/tree/stakeholder-consultation-D7-1 and changes regularly. See the Directory of published versions

## Logical Model: Imaging study model

Official URL: http://www.xt-ehr.eu/fhir/models/StructureDefinition/EHDSImagingStudy | Version: 0.2.1
Draft as of 2026-02-09 | Computable Name: EHDSImagingStudy

Imaging study model includes the key information about the content of an imaging study. It does not include image pixels but includes location pointers to its image content and organises this information according to the well-established model of an imaging study made of one or more series and each series made of instances or images. Composed of a set of data (DICOM KOS) that facilitates the location of all available images.

Usages:

- Use this Logical Model: Imaging report model and Observation model

You can also check for usages in the FHIR IG Statistics

### Formal Views of Profile Content

Description of Profiles, Differentials, Snapshots and how the different presentations work.

- Key Elements Table
- Differential Table
- Snapshot Table
- Statistics/References
- All

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
EHDSImagingStudy |  | 0..* | EHDSDataSet | Imaging study model Elements defined in Ancestors:header
header |  | 1..1 | Base | Basic metadata for this information
subject |  | 1..1 | EHDSPatient | Patient/subject information
identifier |  | 1..* | Identifier | Identifiers for the imaging study such as DICOM Study Instance UID. If one or more series elements are present in the imaging study, then there shall be one DICOM Study UID identifier.
author[x] |  | 1..* |  | Author(s) responsible for the provided information.
authorEHDSHealthProfessional |  |  | EHDSHealthProfessional |
authorEHDSOrganisation |  |  | EHDSOrganisation |
authorEHDSDevice |  |  | EHDSDevice |
date |  | 1..1 | dateTime | Date and optionally time of authoring/issuing
status |  | 1..1 | CodeableConcept | Status of the resource or document
language |  | 0..1 | CodeableConcept | Language in which the resource is written. Language is expressed by the IETF language tag. Binding Description: (preferred): BCP 47
modality |  | 0..* | CodeableConcept | All of the distinct values for series' modalities Binding Description: (preferred): DICOM CID 33 Modality
bodySite |  | 0..* | EHDSBodyStructure | All of the distinct values for series' examined body parts.
encounter |  | 0..1 | EHDSEncounter | Reference to the encounter with which this imaging study is associated
started |  | 0..1 | dateTime | Date and time the study started.
basedOn |  | 0..* | EHDSServiceRequest | References to the diagnostic requests that resulted in this imaging study being performed.
numberOfSeries |  | 0..1 | integer | Number of series in the study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
numberOfInstances |  | 0..1 | integer | Number of service-object pair (SOP) instances in the study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
description |  | 0..1 | string | The imaging manager description of the study. Institution-generated description or classification of the study (component) performed.
studyCustodian |  | 0..1 | EHDSOrganisation | Organisation name, address, contact information.
studyEndpoint |  | 0..1 | EHDSEndpoint | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
series |  | 0..* | Base | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
seriesUid |  | 1..1 | Identifier | DICOM Series Instance UID for the series
number |  | 0..1 | integer | Numeric identifier of this series
seriesModality |  | 1..1 | CodeableConcept | Acquisition modality - the modality used for this series Binding Description: (preferred): DICOM CID 29 Acquisition Modality
description |  | 0..1 | string | A short human readable summary of the series
numberOfInstances |  | 0..1 | integer | Number of series related instances
seriesEndpoint |  | 0..1 | EHDSEndpoint | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
bodySite |  | 0..1 | EHDSBodyStructure | Body part (with laterality) examined
specimen |  | 0..* | EHDSSpecimen | Specimen imaged
started |  | 0..1 | dateTime | When the series started
instancesInTheSeries |  | 0..* | Base | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
instanceTitle |  | 0..1 | string | Instance title that is the description of the instance.
instanceUid |  | 1..1 | Identifier | DICOM SOP Instance UID
sopClass |  | 1..1 | uri | SOP class - DICOM class type
instanceNumber |  | 0..1 | integer | The number of this instance in the series
numberOfFrames |  | 0..1 | integer | The number of frames in a multiframe instance
keyImage |  | 0..* | Base | List of key image flags with a reason why this image is selected as a key image, and reference to the Key Image Note that flags the image as significant within the Imaging Study Manifest
flag |  | 1..1 | CodeableConcept | Reason for flagging the image as significant Binding Description: (preferred): DICOM PS3.16 in Table CID 7010
reason |  | 0..1 | string | Textual reason for flagging the image as significant
seriesUID |  | 1..* | Identifier | Series instance UID for the series that contains the instances flagged as significant
instanceUID |  | 1..* | Identifier | SOP Instance UID for the instances flagged as significant by the Key Image Note object (DICOM KOS) that flags this image
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
EHDSImagingStudy.header.​language | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.modality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​seriesModality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​instancesInTheSeries.​keyImage.flag | Base | preferred |  | Not State | Unknown

This structure is derived from EHDSDataSet

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
EHDSImagingStudy |  | 0..* | EHDSDataSet | Imaging study model Elements defined in Ancestors:header
header |  |  |  |
identifier |  | 1..* | Identifier | Identifiers for the imaging study such as DICOM Study Instance UID. If one or more series elements are present in the imaging study, then there shall be one DICOM Study UID identifier.
author[x] |  | 1..* | EHDSHealthProfessional, EHDSOrganisation, EHDSDevice | Author(s) responsible for the provided information.
date |  | 1..1 | dateTime | Date and optionally time of authoring/issuing
source |  | 0..0 |  | Source of information (e.g. patient, patient's proxy). Used in case the patient has authored the information or the author has submitted patient-stated information.
modality |  | 0..* | CodeableConcept | All of the distinct values for series' modalities Binding Description: (preferred): DICOM CID 33 Modality
bodySite |  | 0..* | EHDSBodyStructure | All of the distinct values for series' examined body parts.
encounter |  | 0..1 | EHDSEncounter | Reference to the encounter with which this imaging study is associated
started |  | 0..1 | dateTime | Date and time the study started.
basedOn |  | 0..* | EHDSServiceRequest | References to the diagnostic requests that resulted in this imaging study being performed.
numberOfSeries |  | 0..1 | integer | Number of series in the study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
numberOfInstances |  | 0..1 | integer | Number of service-object pair (SOP) instances in the study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
description |  | 0..1 | string | The imaging manager description of the study. Institution-generated description or classification of the study (component) performed.
studyCustodian |  | 0..1 | EHDSOrganisation | Organisation name, address, contact information.
studyEndpoint |  | 0..1 | EHDSEndpoint | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
series |  | 0..* | Base | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
seriesUid |  | 1..1 | Identifier | DICOM Series Instance UID for the series
number |  | 0..1 | integer | Numeric identifier of this series
seriesModality |  | 1..1 | CodeableConcept | Acquisition modality - the modality used for this series Binding Description: (preferred): DICOM CID 29 Acquisition Modality
description |  | 0..1 | string | A short human readable summary of the series
numberOfInstances |  | 0..1 | integer | Number of series related instances
seriesEndpoint |  | 0..1 | EHDSEndpoint | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
bodySite |  | 0..1 | EHDSBodyStructure | Body part (with laterality) examined
specimen |  | 0..* | EHDSSpecimen | Specimen imaged
started |  | 0..1 | dateTime | When the series started
instancesInTheSeries |  | 0..* | Base | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
instanceTitle |  | 0..1 | string | Instance title that is the description of the instance.
instanceUid |  | 1..1 | Identifier | DICOM SOP Instance UID
sopClass |  | 1..1 | uri | SOP class - DICOM class type
instanceNumber |  | 0..1 | integer | The number of this instance in the series
numberOfFrames |  | 0..1 | integer | The number of frames in a multiframe instance
keyImage |  | 0..* | Base | List of key image flags with a reason why this image is selected as a key image, and reference to the Key Image Note that flags the image as significant within the Imaging Study Manifest
flag |  | 1..1 | CodeableConcept | Reason for flagging the image as significant Binding Description: (preferred): DICOM PS3.16 in Table CID 7010
reason |  | 0..1 | string | Textual reason for flagging the image as significant
seriesUID |  | 1..* | Identifier | Series instance UID for the series that contains the instances flagged as significant
instanceUID |  | 1..* | Identifier | SOP Instance UID for the instances flagged as significant by the Key Image Note object (DICOM KOS) that flags this image
Documentation for this format

#### Terminology Bindings (Differential)

Path | Status | Usage | ValueSet | Version | Source
EHDSImagingStudy.modality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​seriesModality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​instancesInTheSeries.​keyImage.flag | Base | preferred |  | Not State | Unknown

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
EHDSImagingStudy |  | 0..* | EHDSDataSet | Imaging study model Elements defined in Ancestors:header
header |  | 1..1 | Base | Basic metadata for this information
subject |  | 1..1 | EHDSPatient | Patient/subject information
identifier |  | 1..* | Identifier | Identifiers for the imaging study such as DICOM Study Instance UID. If one or more series elements are present in the imaging study, then there shall be one DICOM Study UID identifier.
author[x] |  | 1..* |  | Author(s) responsible for the provided information.
authorEHDSHealthProfessional |  |  | EHDSHealthProfessional |
authorEHDSOrganisation |  |  | EHDSOrganisation |
authorEHDSDevice |  |  | EHDSDevice |
date |  | 1..1 | dateTime | Date and optionally time of authoring/issuing
status |  | 1..1 | CodeableConcept | Status of the resource or document
language |  | 0..1 | CodeableConcept | Language in which the resource is written. Language is expressed by the IETF language tag. Binding Description: (preferred): BCP 47
modality |  | 0..* | CodeableConcept | All of the distinct values for series' modalities Binding Description: (preferred): DICOM CID 33 Modality
bodySite |  | 0..* | EHDSBodyStructure | All of the distinct values for series' examined body parts.
encounter |  | 0..1 | EHDSEncounter | Reference to the encounter with which this imaging study is associated
started |  | 0..1 | dateTime | Date and time the study started.
basedOn |  | 0..* | EHDSServiceRequest | References to the diagnostic requests that resulted in this imaging study being performed.
numberOfSeries |  | 0..1 | integer | Number of series in the study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
numberOfInstances |  | 0..1 | integer | Number of service-object pair (SOP) instances in the study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
description |  | 0..1 | string | The imaging manager description of the study. Institution-generated description or classification of the study (component) performed.
studyCustodian |  | 0..1 | EHDSOrganisation | Organisation name, address, contact information.
studyEndpoint |  | 0..1 | EHDSEndpoint | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
series |  | 0..* | Base | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
seriesUid |  | 1..1 | Identifier | DICOM Series Instance UID for the series
number |  | 0..1 | integer | Numeric identifier of this series
seriesModality |  | 1..1 | CodeableConcept | Acquisition modality - the modality used for this series Binding Description: (preferred): DICOM CID 29 Acquisition Modality
description |  | 0..1 | string | A short human readable summary of the series
numberOfInstances |  | 0..1 | integer | Number of series related instances
seriesEndpoint |  | 0..1 | EHDSEndpoint | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
bodySite |  | 0..1 | EHDSBodyStructure | Body part (with laterality) examined
specimen |  | 0..* | EHDSSpecimen | Specimen imaged
started |  | 0..1 | dateTime | When the series started
instancesInTheSeries |  | 0..* | Base | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
instanceTitle |  | 0..1 | string | Instance title that is the description of the instance.
instanceUid |  | 1..1 | Identifier | DICOM SOP Instance UID
sopClass |  | 1..1 | uri | SOP class - DICOM class type
instanceNumber |  | 0..1 | integer | The number of this instance in the series
numberOfFrames |  | 0..1 | integer | The number of frames in a multiframe instance
keyImage |  | 0..* | Base | List of key image flags with a reason why this image is selected as a key image, and reference to the Key Image Note that flags the image as significant within the Imaging Study Manifest
flag |  | 1..1 | CodeableConcept | Reason for flagging the image as significant Binding Description: (preferred): DICOM PS3.16 in Table CID 7010
reason |  | 0..1 | string | Textual reason for flagging the image as significant
seriesUID |  | 1..* | Identifier | Series instance UID for the series that contains the instances flagged as significant
instanceUID |  | 1..* | Identifier | SOP Instance UID for the instances flagged as significant by the Key Image Note object (DICOM KOS) that flags this image
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
EHDSImagingStudy.header.​language | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.modality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​seriesModality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​instancesInTheSeries.​keyImage.flag | Base | preferred |  | Not State | Unknown

This structure is derived from EHDSDataSet

Summary

Mandatory: 3 elements(7 nested mandatory elements)
Prohibited: 1 element

Key Elements View

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
EHDSImagingStudy |  | 0..* | EHDSDataSet | Imaging study model Elements defined in Ancestors:header
header |  | 1..1 | Base | Basic metadata for this information
subject |  | 1..1 | EHDSPatient | Patient/subject information
identifier |  | 1..* | Identifier | Identifiers for the imaging study such as DICOM Study Instance UID. If one or more series elements are present in the imaging study, then there shall be one DICOM Study UID identifier.
author[x] |  | 1..* |  | Author(s) responsible for the provided information.
authorEHDSHealthProfessional |  |  | EHDSHealthProfessional |
authorEHDSOrganisation |  |  | EHDSOrganisation |
authorEHDSDevice |  |  | EHDSDevice |
date |  | 1..1 | dateTime | Date and optionally time of authoring/issuing
status |  | 1..1 | CodeableConcept | Status of the resource or document
language |  | 0..1 | CodeableConcept | Language in which the resource is written. Language is expressed by the IETF language tag. Binding Description: (preferred): BCP 47
modality |  | 0..* | CodeableConcept | All of the distinct values for series' modalities Binding Description: (preferred): DICOM CID 33 Modality
bodySite |  | 0..* | EHDSBodyStructure | All of the distinct values for series' examined body parts.
encounter |  | 0..1 | EHDSEncounter | Reference to the encounter with which this imaging study is associated
started |  | 0..1 | dateTime | Date and time the study started.
basedOn |  | 0..* | EHDSServiceRequest | References to the diagnostic requests that resulted in this imaging study being performed.
numberOfSeries |  | 0..1 | integer | Number of series in the study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
numberOfInstances |  | 0..1 | integer | Number of service-object pair (SOP) instances in the study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
description |  | 0..1 | string | The imaging manager description of the study. Institution-generated description or classification of the study (component) performed.
studyCustodian |  | 0..1 | EHDSOrganisation | Organisation name, address, contact information.
studyEndpoint |  | 0..1 | EHDSEndpoint | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
series |  | 0..* | Base | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
seriesUid |  | 1..1 | Identifier | DICOM Series Instance UID for the series
number |  | 0..1 | integer | Numeric identifier of this series
seriesModality |  | 1..1 | CodeableConcept | Acquisition modality - the modality used for this series Binding Description: (preferred): DICOM CID 29 Acquisition Modality
description |  | 0..1 | string | A short human readable summary of the series
numberOfInstances |  | 0..1 | integer | Number of series related instances
seriesEndpoint |  | 0..1 | EHDSEndpoint | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
bodySite |  | 0..1 | EHDSBodyStructure | Body part (with laterality) examined
specimen |  | 0..* | EHDSSpecimen | Specimen imaged
started |  | 0..1 | dateTime | When the series started
instancesInTheSeries |  | 0..* | Base | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
instanceTitle |  | 0..1 | string | Instance title that is the description of the instance.
instanceUid |  | 1..1 | Identifier | DICOM SOP Instance UID
sopClass |  | 1..1 | uri | SOP class - DICOM class type
instanceNumber |  | 0..1 | integer | The number of this instance in the series
numberOfFrames |  | 0..1 | integer | The number of frames in a multiframe instance
keyImage |  | 0..* | Base | List of key image flags with a reason why this image is selected as a key image, and reference to the Key Image Note that flags the image as significant within the Imaging Study Manifest
flag |  | 1..1 | CodeableConcept | Reason for flagging the image as significant Binding Description: (preferred): DICOM PS3.16 in Table CID 7010
reason |  | 0..1 | string | Textual reason for flagging the image as significant
seriesUID |  | 1..* | Identifier | Series instance UID for the series that contains the instances flagged as significant
instanceUID |  | 1..* | Identifier | SOP Instance UID for the instances flagged as significant by the Key Image Note object (DICOM KOS) that flags this image
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
EHDSImagingStudy.header.​language | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.modality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​seriesModality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​instancesInTheSeries.​keyImage.flag | Base | preferred |  | Not State | Unknown

Differential View

This structure is derived from EHDSDataSet

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
EHDSImagingStudy |  | 0..* | EHDSDataSet | Imaging study model Elements defined in Ancestors:header
header |  |  |  |
identifier |  | 1..* | Identifier | Identifiers for the imaging study such as DICOM Study Instance UID. If one or more series elements are present in the imaging study, then there shall be one DICOM Study UID identifier.
author[x] |  | 1..* | EHDSHealthProfessional, EHDSOrganisation, EHDSDevice | Author(s) responsible for the provided information.
date |  | 1..1 | dateTime | Date and optionally time of authoring/issuing
source |  | 0..0 |  | Source of information (e.g. patient, patient's proxy). Used in case the patient has authored the information or the author has submitted patient-stated information.
modality |  | 0..* | CodeableConcept | All of the distinct values for series' modalities Binding Description: (preferred): DICOM CID 33 Modality
bodySite |  | 0..* | EHDSBodyStructure | All of the distinct values for series' examined body parts.
encounter |  | 0..1 | EHDSEncounter | Reference to the encounter with which this imaging study is associated
started |  | 0..1 | dateTime | Date and time the study started.
basedOn |  | 0..* | EHDSServiceRequest | References to the diagnostic requests that resulted in this imaging study being performed.
numberOfSeries |  | 0..1 | integer | Number of series in the study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
numberOfInstances |  | 0..1 | integer | Number of service-object pair (SOP) instances in the study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
description |  | 0..1 | string | The imaging manager description of the study. Institution-generated description or classification of the study (component) performed.
studyCustodian |  | 0..1 | EHDSOrganisation | Organisation name, address, contact information.
studyEndpoint |  | 0..1 | EHDSEndpoint | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
series |  | 0..* | Base | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
seriesUid |  | 1..1 | Identifier | DICOM Series Instance UID for the series
number |  | 0..1 | integer | Numeric identifier of this series
seriesModality |  | 1..1 | CodeableConcept | Acquisition modality - the modality used for this series Binding Description: (preferred): DICOM CID 29 Acquisition Modality
description |  | 0..1 | string | A short human readable summary of the series
numberOfInstances |  | 0..1 | integer | Number of series related instances
seriesEndpoint |  | 0..1 | EHDSEndpoint | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
bodySite |  | 0..1 | EHDSBodyStructure | Body part (with laterality) examined
specimen |  | 0..* | EHDSSpecimen | Specimen imaged
started |  | 0..1 | dateTime | When the series started
instancesInTheSeries |  | 0..* | Base | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
instanceTitle |  | 0..1 | string | Instance title that is the description of the instance.
instanceUid |  | 1..1 | Identifier | DICOM SOP Instance UID
sopClass |  | 1..1 | uri | SOP class - DICOM class type
instanceNumber |  | 0..1 | integer | The number of this instance in the series
numberOfFrames |  | 0..1 | integer | The number of frames in a multiframe instance
keyImage |  | 0..* | Base | List of key image flags with a reason why this image is selected as a key image, and reference to the Key Image Note that flags the image as significant within the Imaging Study Manifest
flag |  | 1..1 | CodeableConcept | Reason for flagging the image as significant Binding Description: (preferred): DICOM PS3.16 in Table CID 7010
reason |  | 0..1 | string | Textual reason for flagging the image as significant
seriesUID |  | 1..* | Identifier | Series instance UID for the series that contains the instances flagged as significant
instanceUID |  | 1..* | Identifier | SOP Instance UID for the instances flagged as significant by the Key Image Note object (DICOM KOS) that flags this image
Documentation for this format

#### Terminology Bindings (Differential)

Path | Status | Usage | ValueSet | Version | Source
EHDSImagingStudy.modality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​seriesModality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​instancesInTheSeries.​keyImage.flag | Base | preferred |  | Not State | Unknown

Snapshot View

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
EHDSImagingStudy |  | 0..* | EHDSDataSet | Imaging study model Elements defined in Ancestors:header
header |  | 1..1 | Base | Basic metadata for this information
subject |  | 1..1 | EHDSPatient | Patient/subject information
identifier |  | 1..* | Identifier | Identifiers for the imaging study such as DICOM Study Instance UID. If one or more series elements are present in the imaging study, then there shall be one DICOM Study UID identifier.
author[x] |  | 1..* |  | Author(s) responsible for the provided information.
authorEHDSHealthProfessional |  |  | EHDSHealthProfessional |
authorEHDSOrganisation |  |  | EHDSOrganisation |
authorEHDSDevice |  |  | EHDSDevice |
date |  | 1..1 | dateTime | Date and optionally time of authoring/issuing
status |  | 1..1 | CodeableConcept | Status of the resource or document
language |  | 0..1 | CodeableConcept | Language in which the resource is written. Language is expressed by the IETF language tag. Binding Description: (preferred): BCP 47
modality |  | 0..* | CodeableConcept | All of the distinct values for series' modalities Binding Description: (preferred): DICOM CID 33 Modality
bodySite |  | 0..* | EHDSBodyStructure | All of the distinct values for series' examined body parts.
encounter |  | 0..1 | EHDSEncounter | Reference to the encounter with which this imaging study is associated
started |  | 0..1 | dateTime | Date and time the study started.
basedOn |  | 0..* | EHDSServiceRequest | References to the diagnostic requests that resulted in this imaging study being performed.
numberOfSeries |  | 0..1 | integer | Number of series in the study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
numberOfInstances |  | 0..1 | integer | Number of service-object pair (SOP) instances in the study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
description |  | 0..1 | string | The imaging manager description of the study. Institution-generated description or classification of the study (component) performed.
studyCustodian |  | 0..1 | EHDSOrganisation | Organisation name, address, contact information.
studyEndpoint |  | 0..1 | EHDSEndpoint | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
series |  | 0..* | Base | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
seriesUid |  | 1..1 | Identifier | DICOM Series Instance UID for the series
number |  | 0..1 | integer | Numeric identifier of this series
seriesModality |  | 1..1 | CodeableConcept | Acquisition modality - the modality used for this series Binding Description: (preferred): DICOM CID 29 Acquisition Modality
description |  | 0..1 | string | A short human readable summary of the series
numberOfInstances |  | 0..1 | integer | Number of series related instances
seriesEndpoint |  | 0..1 | EHDSEndpoint | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
bodySite |  | 0..1 | EHDSBodyStructure | Body part (with laterality) examined
specimen |  | 0..* | EHDSSpecimen | Specimen imaged
started |  | 0..1 | dateTime | When the series started
instancesInTheSeries |  | 0..* | Base | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
instanceTitle |  | 0..1 | string | Instance title that is the description of the instance.
instanceUid |  | 1..1 | Identifier | DICOM SOP Instance UID
sopClass |  | 1..1 | uri | SOP class - DICOM class type
instanceNumber |  | 0..1 | integer | The number of this instance in the series
numberOfFrames |  | 0..1 | integer | The number of frames in a multiframe instance
keyImage |  | 0..* | Base | List of key image flags with a reason why this image is selected as a key image, and reference to the Key Image Note that flags the image as significant within the Imaging Study Manifest
flag |  | 1..1 | CodeableConcept | Reason for flagging the image as significant Binding Description: (preferred): DICOM PS3.16 in Table CID 7010
reason |  | 0..1 | string | Textual reason for flagging the image as significant
seriesUID |  | 1..* | Identifier | Series instance UID for the series that contains the instances flagged as significant
instanceUID |  | 1..* | Identifier | SOP Instance UID for the instances flagged as significant by the Key Image Note object (DICOM KOS) that flags this image
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
EHDSImagingStudy.header.​language | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.modality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​seriesModality | Base | preferred |  | Not State | Unknown
EHDSImagingStudy.series.​instancesInTheSeries.​keyImage.flag | Base | preferred |  | Not State | Unknown

This structure is derived from EHDSDataSet

Summary

Mandatory: 3 elements(7 nested mandatory elements)
Prohibited: 1 element

Other representations of profile: CSV, Excel