EHDS Logical Information Models
0.1.0 - ci-build

EHDS Logical Information Models, published by Xt-EHR. This guide is not an authorized publication; it is the continuous build for version 0.1.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/Xt-EHR/xt-ehr-common/tree/stakeholder-consultation-D7-3 and changes regularly. See the Directory of published versions

## Logical Model: EHDSImagingStudy - Detailed Descriptions

Draft as of 2025-08-25

Definitions for the EHDSImagingStudy logical model.

- Key Elements Table
- Differential Elements Table
- Snapshot Elements Table

Guidance on how to interpret the contents of this table can be foundhere

0. EHDSImagingStudy
Definition | EHDS refined base model for Imaging study Base definition for all types defined in FHIR type system.
Short | Imaging study modelBase for all types and resources
Control | 0..*
Is Modifier | false
Logical Model | Instances of this logical model are not marked to be the target of a Reference
2. EHDSImagingStudy.header
Definition | Common header for all patient-related data
Short | Common header for all patient-related data
Control | 1..1
Type | Base
4. EHDSImagingStudy.header.subject
Definition | Patient/subject information
Short | Subject
Control | 1..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSPatient
6. EHDSImagingStudy.header.identifier
Definition | Business identifier for the object
Short | Identifiers for the Imaging Study such as DICOM Study Instance UID. If one or more series elements are present in the ImagingStudy, then there shall be one DICOM Study UID identifier.
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 1..*
Type | Identifier
Requirements | eHN Guideline IMG (v1.1): B.1.1
8. EHDSImagingStudy.header.authorship
Definition | Resource authoring details
Short | Authorship
Control | 1..*
Type | Base
10. EHDSImagingStudy.header.authorship.author[x]
Definition | Author(s) by whom the resource was/were authored. Multiple authors could be provided.
Short | Author
Control | 1..1
Type | Choice of: https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSHealthProfessional, https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSOrganisation, https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSDevice
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
12. EHDSImagingStudy.header.authorship.datetime
Definition | Date and time of the issuing the document/resource by its author.
Short | Date and time of authoring/issuing
Control | 1..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
14. EHDSImagingStudy.header.lastUpdate
Definition | Date and time of the last update to the document/information
Short | Date and time of the last update to the resource
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
16. EHDSImagingStudy.header.status
Definition | Status of the resource
Short | Status of the resource
Control | 1..1
Type | CodeableConcept
18. EHDSImagingStudy.header.statusReason[x]
Definition | Reason for the current status of the resource.
Short | Reason for the current status of the resource.
Control | 0..1
Type | Choice of: CodeableConcept, string
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
20. EHDSImagingStudy.header.language
Definition | Language in which the resource is written. Language is expressed by the IETF language tag.
Short | Language
Control | 0..1
Binding | BCP 47
Type | CodeableConcept
22. EHDSImagingStudy.header.version
Definition | Business version of the resource.
Short | Version
Note | This is a business version Id, not a resource version Id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
24. EHDSImagingStudy.presentedForm
Definition | A narrative easy-to-read representation of the full data set, e.g. PDF-version of a document
Short | A narrative easy-to-read representation of the full data set, e.g. PDF-version of a document
Control | 0..*
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSAttachment
26. EHDSImagingStudy.modality
Definition | All of the distinct values for series' modalities
Short | All of the distinct values for series' modalities
Control | 0..*
Binding | DICOM CID029
Type | CodeableConcept
28. EHDSImagingStudy.encounter
Definition | Reference to the encounter with which this imaging study is associated
Short | Reference to the encounter with which this imaging study is associated
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSEncounter
30. EHDSImagingStudy.started
Definition | Date and time the study started.
Short | Date and time the study started.
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
32. EHDSImagingStudy.basedOn
Definition | References to the diagnostic requests that resulted in this imaging study being performed.
Short | References to the diagnostic requests that resulted in this imaging study being performed.
Control | 0..*
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSServiceRequest
34. EHDSImagingStudy.numberOfSeries
Definition | Number of Series in the Study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
Short | Number of Series in the Study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
36. EHDSImagingStudy.numberOfInstances
Definition | Number of Service-Object Pairs (SOP) Instances in Study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
Short | Number of Service-Object Pairs (SOP) Instances in Study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
38. EHDSImagingStudy.description
Definition | The Imaging Manager description of the study. Institution-generated description or classification of the Study (component) performed.
Short | The Imaging Manager description of the study. Institution-generated description or classification of the Study (component) performed.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | eHN Guideline IMG (v1.1): B.1.2
40. EHDSImagingStudy.studyCustodian
Definition | Organisation name, address, contact information.
Short | Organisation name, address, contact information.
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSOrganisation
Requirements | eHN Guideline IMG (v1.1): B.1.3
42. EHDSImagingStudy.studyEndpoint
Definition | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Short | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSEndpoint
44. EHDSImagingStudy.series
Definition | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
Short | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
Control | 0..*
Type | Base
Requirements | eHN Guideline IMG (v1.1): B.1.4
46. EHDSImagingStudy.series.seriesUid
Definition | DICOM Series Instance UID for the series
Short | DICOM Series Instance UID for the series
Control | 1..1
Type | Identifier
Requirements | eHN Guideline IMG (v1.1): B.1.4.2
48. EHDSImagingStudy.series.number
Definition | Numeric identifier of this series
Short | Numeric identifier of this series
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
50. EHDSImagingStudy.series.acquisitionModality
Definition | Acquisition modality - the modality used for this series
Short | Acquisition modality - the modality used for this series
Control | 1..1
Binding | DICOM CID029
Type | CodeableConcept
Requirements | eHN Guideline IMG (v1.1): B.1.4.3
52. EHDSImagingStudy.series.description
Definition | A short human readable summary of the series
Short | A short human readable summary of the series
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | eHN Guideline IMG (v1.1): B.1.4.1
54. EHDSImagingStudy.series.numberOfInstances
Definition | Number of Series Related Instances
Short | Number of Series Related Instances
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
56. EHDSImagingStudy.series.seriesEndpoint
Definition | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Short | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSEndpoint
Requirements | eHN Guideline IMG (v1.1): B.1.4.6
58. EHDSImagingStudy.series.bodySite
Definition | Body part (with laterality) examined
Short | Body part (with laterality) examined
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSBodyStructure
60. EHDSImagingStudy.series.specimen
Definition | Specimen imaged
Short | Specimen imaged
Control | 0..*
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSSpecimen
62. EHDSImagingStudy.series.started
Definition | When the series started
Short | When the series started
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
64. EHDSImagingStudy.series.instancesInTheSeries
Definition | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
Short | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
Control | 0..*
Type | Base
Requirements | eHN Guideline IMG (v1.1): B.1.4.7
66. EHDSImagingStudy.series.instancesInTheSeries.instanceTitle
Definition | Instance title that is the description of the instance.
Short | Instance title that is the description of the instance.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
68. EHDSImagingStudy.series.instancesInTheSeries.instanceUid
Definition | DICOM SOP Instance UID
Short | DICOM SOP Instance UID
Control | 1..1
Type | Identifier
Requirements | eHN Guideline IMG (v1.1): B.1.4.7.1
70. EHDSImagingStudy.series.instancesInTheSeries.sopClass
Definition | SOP class - DICOM class type
Short | SOP class - DICOM class type
Control | 1..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | DICOM KOS
72. EHDSImagingStudy.series.instancesInTheSeries.instanceNumber
Definition | The number of this instance in the series
Short | The number of this instance in the series
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | eHN Guideline IMG (v1.1): B.1.4.7.3
74. EHDSImagingStudy.series.instancesInTheSeries.numberOfFrames
Definition | The number of frames in a multiframe instance
Short | The number of frames in a multiframe instance
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | DICOM KOS

Guidance on how to interpret the contents of this table can be foundhere

0. EHDSImagingStudy
Definition | EHDS refined base model for Imaging study
Short | Imaging study model
Logical Model | Instances of this logical model are not marked to be the target of a Reference
2. EHDSImagingStudy.header
4. EHDSImagingStudy.header.identifier
Short | Identifiers for the Imaging Study such as DICOM Study Instance UID. If one or more series elements are present in the ImagingStudy, then there shall be one DICOM Study UID identifier.
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 1..?
Requirements | eHN Guideline IMG (v1.1): B.1.1
6. EHDSImagingStudy.modality
Definition | All of the distinct values for series' modalities
Short | All of the distinct values for series' modalities
Control | 0..*
Binding | DICOM CID029
Type | CodeableConcept
8. EHDSImagingStudy.encounter
Definition | Reference to the encounter with which this imaging study is associated
Short | Reference to the encounter with which this imaging study is associated
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSEncounter
10. EHDSImagingStudy.started
Definition | Date and time the study started.
Short | Date and time the study started.
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
12. EHDSImagingStudy.basedOn
Definition | References to the diagnostic requests that resulted in this imaging study being performed.
Short | References to the diagnostic requests that resulted in this imaging study being performed.
Control | 0..*
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSServiceRequest
14. EHDSImagingStudy.numberOfSeries
Definition | Number of Series in the Study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
Short | Number of Series in the Study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
16. EHDSImagingStudy.numberOfInstances
Definition | Number of Service-Object Pairs (SOP) Instances in Study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
Short | Number of Service-Object Pairs (SOP) Instances in Study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
18. EHDSImagingStudy.description
Definition | The Imaging Manager description of the study. Institution-generated description or classification of the Study (component) performed.
Short | The Imaging Manager description of the study. Institution-generated description or classification of the Study (component) performed.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | eHN Guideline IMG (v1.1): B.1.2
20. EHDSImagingStudy.studyCustodian
Definition | Organisation name, address, contact information.
Short | Organisation name, address, contact information.
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSOrganisation
Requirements | eHN Guideline IMG (v1.1): B.1.3
22. EHDSImagingStudy.studyEndpoint
Definition | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Short | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSEndpoint
24. EHDSImagingStudy.series
Definition | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
Short | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
Control | 0..*
Type | Base
Requirements | eHN Guideline IMG (v1.1): B.1.4
26. EHDSImagingStudy.series.seriesUid
Definition | DICOM Series Instance UID for the series
Short | DICOM Series Instance UID for the series
Control | 1..1
Type | Identifier
Requirements | eHN Guideline IMG (v1.1): B.1.4.2
28. EHDSImagingStudy.series.number
Definition | Numeric identifier of this series
Short | Numeric identifier of this series
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
30. EHDSImagingStudy.series.acquisitionModality
Definition | Acquisition modality - the modality used for this series
Short | Acquisition modality - the modality used for this series
Control | 1..1
Binding | DICOM CID029
Type | CodeableConcept
Requirements | eHN Guideline IMG (v1.1): B.1.4.3
32. EHDSImagingStudy.series.description
Definition | A short human readable summary of the series
Short | A short human readable summary of the series
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | eHN Guideline IMG (v1.1): B.1.4.1
34. EHDSImagingStudy.series.numberOfInstances
Definition | Number of Series Related Instances
Short | Number of Series Related Instances
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
36. EHDSImagingStudy.series.seriesEndpoint
Definition | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Short | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSEndpoint
Requirements | eHN Guideline IMG (v1.1): B.1.4.6
38. EHDSImagingStudy.series.bodySite
Definition | Body part (with laterality) examined
Short | Body part (with laterality) examined
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSBodyStructure
40. EHDSImagingStudy.series.specimen
Definition | Specimen imaged
Short | Specimen imaged
Control | 0..*
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSSpecimen
42. EHDSImagingStudy.series.started
Definition | When the series started
Short | When the series started
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
44. EHDSImagingStudy.series.instancesInTheSeries
Definition | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
Short | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
Control | 0..*
Type | Base
Requirements | eHN Guideline IMG (v1.1): B.1.4.7
46. EHDSImagingStudy.series.instancesInTheSeries.instanceTitle
Definition | Instance title that is the description of the instance.
Short | Instance title that is the description of the instance.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
48. EHDSImagingStudy.series.instancesInTheSeries.instanceUid
Definition | DICOM SOP Instance UID
Short | DICOM SOP Instance UID
Control | 1..1
Type | Identifier
Requirements | eHN Guideline IMG (v1.1): B.1.4.7.1
50. EHDSImagingStudy.series.instancesInTheSeries.sopClass
Definition | SOP class - DICOM class type
Short | SOP class - DICOM class type
Control | 1..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | DICOM KOS
52. EHDSImagingStudy.series.instancesInTheSeries.instanceNumber
Definition | The number of this instance in the series
Short | The number of this instance in the series
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | eHN Guideline IMG (v1.1): B.1.4.7.3
54. EHDSImagingStudy.series.instancesInTheSeries.numberOfFrames
Definition | The number of frames in a multiframe instance
Short | The number of frames in a multiframe instance
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | DICOM KOS

Guidance on how to interpret the contents of this table can be foundhere

0. EHDSImagingStudy
Definition | EHDS refined base model for Imaging study
Short | Imaging study model
Control | 0..*
Is Modifier | false
Logical Model | Instances of this logical model are not marked to be the target of a Reference
2. EHDSImagingStudy.header
Definition | Common header for all patient-related data
Short | Common header for all patient-related data
Control | 1..1
Type | Base
4. EHDSImagingStudy.header.subject
Definition | Patient/subject information
Short | Subject
Control | 1..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSPatient
6. EHDSImagingStudy.header.identifier
Definition | Business identifier for the object
Short | Identifiers for the Imaging Study such as DICOM Study Instance UID. If one or more series elements are present in the ImagingStudy, then there shall be one DICOM Study UID identifier.
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 1..*
Type | Identifier
Requirements | eHN Guideline IMG (v1.1): B.1.1
8. EHDSImagingStudy.header.authorship
Definition | Resource authoring details
Short | Authorship
Control | 1..*
Type | Base
10. EHDSImagingStudy.header.authorship.author[x]
Definition | Author(s) by whom the resource was/were authored. Multiple authors could be provided.
Short | Author
Control | 1..1
Type | Choice of: https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSHealthProfessional, https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSOrganisation, https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSDevice
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
12. EHDSImagingStudy.header.authorship.datetime
Definition | Date and time of the issuing the document/resource by its author.
Short | Date and time of authoring/issuing
Control | 1..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
14. EHDSImagingStudy.header.lastUpdate
Definition | Date and time of the last update to the document/information
Short | Date and time of the last update to the resource
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
16. EHDSImagingStudy.header.status
Definition | Status of the resource
Short | Status of the resource
Control | 1..1
Type | CodeableConcept
18. EHDSImagingStudy.header.statusReason[x]
Definition | Reason for the current status of the resource.
Short | Reason for the current status of the resource.
Control | 0..1
Type | Choice of: CodeableConcept, string
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
20. EHDSImagingStudy.header.language
Definition | Language in which the resource is written. Language is expressed by the IETF language tag.
Short | Language
Control | 0..1
Binding | BCP 47
Type | CodeableConcept
22. EHDSImagingStudy.header.version
Definition | Business version of the resource.
Short | Version
Note | This is a business version Id, not a resource version Id (see discussion)
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
24. EHDSImagingStudy.presentedForm
Definition | A narrative easy-to-read representation of the full data set, e.g. PDF-version of a document
Short | A narrative easy-to-read representation of the full data set, e.g. PDF-version of a document
Control | 0..*
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSAttachment
26. EHDSImagingStudy.modality
Definition | All of the distinct values for series' modalities
Short | All of the distinct values for series' modalities
Control | 0..*
Binding | DICOM CID029
Type | CodeableConcept
28. EHDSImagingStudy.encounter
Definition | Reference to the encounter with which this imaging study is associated
Short | Reference to the encounter with which this imaging study is associated
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSEncounter
30. EHDSImagingStudy.started
Definition | Date and time the study started.
Short | Date and time the study started.
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
32. EHDSImagingStudy.basedOn
Definition | References to the diagnostic requests that resulted in this imaging study being performed.
Short | References to the diagnostic requests that resulted in this imaging study being performed.
Control | 0..*
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSServiceRequest
34. EHDSImagingStudy.numberOfSeries
Definition | Number of Series in the Study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
Short | Number of Series in the Study. This value given may be larger than the number of series elements this Resource contains due to resource availability, security, or other factors. This element should be present if any series elements are present.
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
36. EHDSImagingStudy.numberOfInstances
Definition | Number of Service-Object Pairs (SOP) Instances in Study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
Short | Number of Service-Object Pairs (SOP) Instances in Study. This value given may be larger than the number of instance elements this resource contains due to resource availability, security, or other factors. This element should be present if any instance elements are present.
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
38. EHDSImagingStudy.description
Definition | The Imaging Manager description of the study. Institution-generated description or classification of the Study (component) performed.
Short | The Imaging Manager description of the study. Institution-generated description or classification of the Study (component) performed.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | eHN Guideline IMG (v1.1): B.1.2
40. EHDSImagingStudy.studyCustodian
Definition | Organisation name, address, contact information.
Short | Organisation name, address, contact information.
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSOrganisation
Requirements | eHN Guideline IMG (v1.1): B.1.3
42. EHDSImagingStudy.studyEndpoint
Definition | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Short | Study endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSEndpoint
44. EHDSImagingStudy.series
Definition | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
Short | Series. Each study has one or more series of instances, but they may be absent when no series information needs to be conveyed
Control | 0..*
Type | Base
Requirements | eHN Guideline IMG (v1.1): B.1.4
46. EHDSImagingStudy.series.seriesUid
Definition | DICOM Series Instance UID for the series
Short | DICOM Series Instance UID for the series
Control | 1..1
Type | Identifier
Requirements | eHN Guideline IMG (v1.1): B.1.4.2
48. EHDSImagingStudy.series.number
Definition | Numeric identifier of this series
Short | Numeric identifier of this series
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
50. EHDSImagingStudy.series.acquisitionModality
Definition | Acquisition modality - the modality used for this series
Short | Acquisition modality - the modality used for this series
Control | 1..1
Binding | DICOM CID029
Type | CodeableConcept
Requirements | eHN Guideline IMG (v1.1): B.1.4.3
52. EHDSImagingStudy.series.description
Definition | A short human readable summary of the series
Short | A short human readable summary of the series
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | eHN Guideline IMG (v1.1): B.1.4.1
54. EHDSImagingStudy.series.numberOfInstances
Definition | Number of Series Related Instances
Short | Number of Series Related Instances
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
56. EHDSImagingStudy.series.seriesEndpoint
Definition | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Short | Series endpoint describing the technical details of a location that can be connected to for the delivery/retrieval of information. Sufficient information is required to ensure that a connection can be made securely, and appropriate data transmitted as defined by the endpoint owner. These may be locally hosted services, regional services, or national service.
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSEndpoint
Requirements | eHN Guideline IMG (v1.1): B.1.4.6
58. EHDSImagingStudy.series.bodySite
Definition | Body part (with laterality) examined
Short | Body part (with laterality) examined
Control | 0..1
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSBodyStructure
60. EHDSImagingStudy.series.specimen
Definition | Specimen imaged
Short | Specimen imaged
Control | 0..*
Type | https://www.xt-ehr.eu/specifications/fhir/StructureDefinition/EHDSSpecimen
62. EHDSImagingStudy.series.started
Definition | When the series started
Short | When the series started
Control | 0..1
Type | dateTime
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
64. EHDSImagingStudy.series.instancesInTheSeries
Definition | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
Short | Each series has one or more instances, but they may be absent when no instance information needs to be conveyed
Control | 0..*
Type | Base
Requirements | eHN Guideline IMG (v1.1): B.1.4.7
66. EHDSImagingStudy.series.instancesInTheSeries.instanceTitle
Definition | Instance title that is the description of the instance.
Short | Instance title that is the description of the instance.
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
68. EHDSImagingStudy.series.instancesInTheSeries.instanceUid
Definition | DICOM SOP Instance UID
Short | DICOM SOP Instance UID
Control | 1..1
Type | Identifier
Requirements | eHN Guideline IMG (v1.1): B.1.4.7.1
70. EHDSImagingStudy.series.instancesInTheSeries.sopClass
Definition | SOP class - DICOM class type
Short | SOP class - DICOM class type
Control | 1..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | DICOM KOS
72. EHDSImagingStudy.series.instancesInTheSeries.instanceNumber
Definition | The number of this instance in the series
Short | The number of this instance in the series
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | eHN Guideline IMG (v1.1): B.1.4.7.3
74. EHDSImagingStudy.series.instancesInTheSeries.numberOfFrames
Definition | The number of frames in a multiframe instance
Short | The number of frames in a multiframe instance
Control | 0..1
Type | integer
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Requirements | DICOM KOS